Write-through cache controller Requires 5 x 8-bit SRAMs externally to operate 2 Interrupt controllers (Intel 8259 equivalent) 1 Timer (Intel 8254 equivalent) ISA-bus controller and interface pins Port B logic 8042 keyboard controller emulation Command/data mailbox GateA20 FastReset RTC emulation logic DMA controller emulation Emulation support logic Aleph One CALLAS interface logic ARM interface Cache fill burst re-sequencing ARM bus arbiter Misaligned data assembly Bus I/O drivers and pins