Performance 500KBytes/Sec (using UDP) Network interface 16-bit Electrical isolation Withstands 500VRMS for one minute Safety standards IEC 950, EN60950 MTBF 30,000 hours Environmental performance 0�-40�C, 0%-75% humidity (non-condensing) EMC Designed to EN55022 and/or Vfg243+46 Immunity Designed to EN55024 Parts 2 and 4